**EMERGENCY SHOWER / EYEWASH ANNUAL TEST**

| **Annual Testing Requirements** | | **Unit 1** | **Unit 2** | **Unit 3** | **Unit 4** |
| --- | --- | --- | --- | --- | --- |
| Testing tag is connected to unit and up to date | |  |  |  |  |
| Flushing fluid is at room temperature (between 15o and 35oC) | |  |  |  |  |
| Shower and eye wash control valve remains open | |  |  |  |  |
| Eyewash dust covers are fitted and open automatically on operation | |  |  |  |  |
| Passed eyewash gauge test | |  |  |  |  |
| Minimum eyewash flow rate 1.5L minute at 210kPa | |  |  |  |  |
| Minimum shower flow rate 75.7L minute at 210kPa | |  |  |  |  |
| Flow of water starts within one (1) second | |  |  |  |  |
| Signage is legible and clearly displayed | |  |  |  |  |
| **Comments / Notes:** | | | | | |
|  | | | | | |
|  | | | | | |
|  | | | | | |
|  | | | | | |
|  | | | | | |
| **Building:** |  | | | | |
| **Room:** |  | | | | |
| **Tested by:** |  | | | | |
| **Date:** |  | | | | |